PrinterUtility_EN: Printer configuration

| PrinterUtility_EN 1.1.0

Printer configuration

> The division mainly contains the following functions:

1、Set up the printer's printing Settings; 2、Switch the usb mode; 3、Query firmware version;

1. Configure the network parameters with usb.

Precautions:

1. Before operation, make sure that the port parameters are set correctly and connected to the printer, otherwise the operation is prohibited. Please refer to the "\ref page_1_PortSet" page for port settings.
2. The following describes the BK-T680 as an example (different print settings supported by different printer models).

   - Step 1: Go to the printer settings page and select the item you want to set.

     - After the program starts to connect to the device, enter the printer setting interface.
     - Click the Print Settings button.

   - Step 2: Set and save the printer settings 1）Click each drop-down box to select the print settings you want to make. Different printers support different print settings: BTP-R990, BTP-R880NP, BTP-M300 only support setting paper type and density; BT-T080 supports print settings not supported. The BK-T680 supports setting the paper type, density, presenter mode, and presenter wait time. 2）Click the "+" button in the lower left corner to enter the user-defined printer setting interface. The interface is divided into three columns: setting item, instruction and deletion. Click the plus icon to add the customization, double-click the blank to enter the name of the customization printer setting item to be set, and then click the plus icon in the next line to add a new line to set the option name and corresponding instructions. If you want to delete an item, just click the minus sign Icon in the third column. After setting, click the Save button in the lower right corner, and the customized settings will be loaded into the printer setting interface. 3）Click the settings button in the lower right corner to save the current print settings.

3. USB mode switch

   - 1)Click the button to enter the USB mode setting interface. If the current connection mode of the printer is USB, the system will display the USB mode of the currently connected printer. To switch to another USB mode, click the switch button, wait for the following prompt that the conversion is successful, and then restart the printer to make the conversion effective. If the current connection mode of the printer is not USB, the USB mode will not be displayed. Click the switch button Button flyout is not supported.
   - 2）The function is valid only in usb communication, and other communication will remind the function not support.

4. Query firmware version number

   - 1）Click the firmware version number button to pop up the firmware version number of the currently connected printer when the printer is not connected with parallel port and driver; if the current printer is connected with parallel port or driver, pop-up display is not supported temporarily.
5. Configure the network parameters with usb

   - 1）After entering the usb configuration network interface, the parameter information of the current network board is read from the printer, and the first page is the wlan setting relevant item, the second page is the network port IP and the port setting item.

   - 2）In the mode Ad-Hoc mode, the ssid and password can be configured, and the printer parameters should be restarted after the Settings are set. In the infrastructure mode, all parameters are configurable, and the same restart parameters come into force.
   - 3）If the search is restored by default, all the Settings are restored to the default factory value.

   - 4）The function is valid only in usb communication, and other communication will remind the function not support.

   - 5）All embedded models (such as the BK series of BT series printers) will not be able to hold this function, and will also be a warning to the function.

Precautions:

1. When the printer is BK-T680, the presenter wait time can be set only when the presenter mode selects "presenter open, retract", "continue, retract (file send)", "continue, retract (file hold)".
2. The printer settings may not be valid when you print your own samples.